IT 125-41194

Alex Arnold

4-21-25

Lab 13.3.12

Part 1: Create a new WLAN

Step 1: Create a new VLAN interface.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

Step 2: Configure the WLC to use a RADIUS server.

A screenshot of a computer

AI-generated content may be incorrect.

Step 3: Create a new WLAN.

A screenshot of a computer

AI-generated content may be incorrect.

Make it refer to its self for DHCP

A screenshot of a computer

AI-generated content may be incorrect.

Set up DHCP scope

Step 2: Configure SNMP

A screenshot of a computer

AI-generated content may be incorrect.

Part 3: Connect Hosts to the Network

Step 1: Configure a host to connect to the enterprise network.

A screenshot of a computer

AI-generated content may be incorrect.

A computer screen shot of a computer

AI-generated content may be incorrect.

Wireless host connected

A computer screen shot of a black screen

AI-generated content may be incorrect.

Pings to WLC-1 and Radius server pass