IT 125-41194

Alex Arnold

5-5-25

Part 1: Configure IPv4 Static and Floating Static Default Routes

Step 1: Configure an IPv4 static default route.

A black text on a white background

AI-generated content may be incorrect.

Step 2: Configure an IPv4 floating static default route.



Part 2: Configure IPv6 Static and Floating Static Default Routes



Part 3: Configure IPv4 Static and Floating Static Routes to the Internal LANs

Step 1: Configure IPv4 static routes to the internal LANs.

A number with black text

AI-generated content may be incorrect.

Step 2: Configure IPv6 floating static routes to the internal LANs.



Part 4: Configure IPv6 Static and Floating Static Routes to the Internal LANs.

Step 1: Configure IPv6 static routes to the internal LANs.

A black and white text

AI-generated content may be incorrect.

Step 2: Configure IPv6 floating static routes to the internal LANs.



Part 5: Configure Host Routes

Step 1: Configure IPv4 host routes



Step 2: Configure IPv6 host routes.

