IT 125-41194

Alex Arnold

Lab 3.3.12

Part 2 - Step 2

A screenshot of a computer

AI-generated content may be incorrect.

Show the VLAN information after Part 3 - Step 2, and provide screenshot

A screenshot of a computer

AI-generated content may be incorrect.

Show the VLAN information after Part 3 - Step 4, and provide screenshot

Although the access ports are assigned to the appropriate VLANs, were the pings successful? Explain.

This was unsuccessful as the trunk line connecting S2 > S1 and S1 > S3 are still on VLAN 1 so they are unable to communicate to each other as there is no continuous VLAN to traverse.

What could be done to resolve this issue?

To resolve this issue S1 needs to have G0/1 and G0/2 configured as trunks.