IT 125-41194

Alex Arnold

4-21-25

Lab 13.1.10

Part 1: Connect to a Wireless Router

Step 1: Connect Admin to WR.

A diagram of a computer network

AI-generated content may be incorrect.

Step 2: Configure Admin to use DHCP.

A screenshot of a computer


AI-generated content may be incorrect.


**Step 3: Connect to the WR Web Interface.**

A screenshot of a computer

AI-generated content may be incorrect.

Step 4: Configure the Internet Port of WR.





Settings verification

Part 2: Configure the Wireless Settings

Step 1: Configure the WR SSID.

A screenshot of a computer

AI-generated content may be incorrect.

Step 2: Configure wireless security settings.

A screenshot of a computer

AI-generated content may be incorrect.

Step 3: Connect the Wireless Clients.

A screenshot of a computer

AI-generated content may be incorrect.

Laptop 1

A screenshot of a computer

AI-generated content may be incorrect.

Laptop 2

Part 3: Connect Wireless Clients to an Access Point

Step 1: Configure the Access Point.

A screenshot of a computer

AI-generated content may be incorrect.

Step 2: Connect the Wireless Clients.

A screenshot of a computer

AI-generated content may be incorrect.

Laptop 3

A diagram of a network

AI-generated content may be incorrect.

Network map with all devices connected

Part 4: Other Administrative Tasks

Step 1: Change the WR Access Password.

A screenshot of a login box

AI-generated content may be incorrect.

Step 2: Change the DHCP address range in WR.

A screenshot of a computer

AI-generated content may be incorrect.

A screen shot of a computer

AI-generated content may be incorrect.

New ip for admin pc

A screenshot of a computer

AI-generated content may be incorrect.

Laptop 2 connection good

A screenshot of a computer

AI-generated content may be incorrect.

Laptop 3 connection good